If you want to manually load or unload a driver, use modprobe with the -i option to load or insert the module and the -r option to remove or unload the module. The -n, --dry-run, or --show option shows you what will be done, without doing it. You usually use the -v option with these to see more information

Dry run is used to test only. It does not actually do anything